

3918 Cooper Inspection Repairs Made:



Repaired: Removed surface corrosion and added bushing clamp:




Repaired: Installed additional GFCI receptacles




Repaired holes in wall / baseboard:




Repaired: Replaced receptacle with GFI protected receptacle




Repaired:

Moss washed / removed from roof

Gutters cleaned of leaves/debris (however, during fall, leaves collect in gutter)

****

Repaired: Vegetation removed from exterior walls



Repaired: There was no leakage in the drain line, however, the duct tape was removed and drain line repaired with flexible coupling

 ****